
**Z100-0db Bios v191 upgrade steps**

1. Preparation
2. Disable the ME State


Pressing “delete” key of keyboard while power on Z100-0dB to go to bios settings interface.

Goto “advanced page and click “Ctrl+F1” to show hidden option.Disable the ME State by path: Advanced->PCH-FM Configuration->ME State->Disable



Disable ME State

Pressing F4 and click “Yes” to save the settings and restart.




Save Bios settings changing

1. Upgrade Bios
2. Boot the NEO Z100-0dB and the Windows OS.
3. Under Windows OS, extract the BIOS files and copy them to a random folder
4. Check the MD5 value of the AD0J0.191.bin, it should be

MD5: 75D2790F78DF1EDDFE06FE2A8AA06807

SHA1: 97312CAD0EB7A993E1941D571E14DC26C0E07419

1. Right-click the 'FlashBIOS.bat' file, choose 'Run as Administrator'.



1. The Bios will be updated automatically
2. Devices will restart after updated.

Please note, it takes more time than usual for the device to boot up, as it's the first time of booting up after updating the BIOS.